ICAO Codes for 5676V & 734NK

You can set these all up in Foreflight and here are the recommended codes and explanation in the order they are presented in Foreflight under Aircraft/Filing

FAA Equipment

**/G** GPS/GNSS with enroute, terminal, and approach capability

ICAO Equipment Codes

**​B**LPV Approach capability

**G** GNSS type capability

**R** PBN approved means we have the of performance based navigation defined below​

​**S** VOR/VHF/ILS capability (All)

**Y** VHF 8.33 spacing means we have 3 digits com capability after whole number not just 2

**D** DME (Add this code only for 5676V)

​ICAO Surveillance

​**B1** ADSB Out capability

**C** Modes A and C

ICAO Wake Category

**L** for Light

ICAO PBN

**D2** means we have RNAV 1 capability (can track courses within 1 mile 95% of the time)

This also means you are eligible to file and receive RNAV SIDS and STARS